EclerPLEX Release Notes, v1.03r23, 03 Aug 2026

Changes from last version, v1.03r21, 28 Jul 2026:

--------------------------------------------------------

Resolved software/firmware issues:

- Resolved an issue where audio inputs on hot-plugged BIOs did not respond until VIVO was rebooted.
- Fixed a false "Dante is not licensed" notification shown during startup on VIVOs with Dante.


###########################################################################################################


EclerPLEX Release Notes, v1.03r21, 28 Jul 2026
 
Changes from last version, v1.02r24, 12 Jun 2026:

--------------------------------------------------------
 
New features:

- New VIVO/BIO models support: The system now supports the entire range of VIVOs and BIOs, with a variable number of audio and control ports per module. 
- Port numbering: Default port labels and indexes have been updated to use a combined BIO index and port index for accurate addressing across all connected hardware.
- Internal ports have been moved to a dedicated tab for improved navigation and clarity.
- VIVO without Dante support: Added support for VIVO units without a Dante module, including correct handling of Dante LED indicators and error reporting for these configurations.
- Signal Detector: New Signal Detector DSP block that can be linked to a VGPI and used as an event trigger or to monitor signal present value using a panel LED.
- DSP chain editing: Improved paste and insert behavior for DSP blocks within a chain, including the ability to insert a copied block at the beginning of a chain.
- Resize using all handles: Panel objects can now be resized from all 4 sides and all 4 corners, providing full control over object dimensions.
- Button objects as event triggers: Button panel objects can now be configured to trigger events directly, expanding the range of event types accessible from panel controls.
- Panel VU meters can now target VU meters of individual audio ports directly, including inputs, outputs and internal ports.
- GPI values are now displayed in the path selector, making them easier to identify when configuring Events or Panels.

--------------------------------------------------------
 
Resolved software/firmware issues:

- Resolved a 1 dB gain offset that could occur between an input and an output in the DSP signal path.
- Cloud Sync datetime displayed on VIVO LCD now shows "---" when the device has not yet synchronized with EclerCLOUD, instead of showing an incorrect or empty value.
- GPI-triggered events were being executed regardless of their "On boot-up" flag value; this has now been corrected.
- Improved Source selector control events to prevent unexpected jumps between selected inputs when using a WPaVOL-SR as a trigger.
- Color picker dialog now displays HEX codes correctly and Copy/Paste functions work as expected.
- Resolved an issue where text input fields could unexpectedly lose focus, causing typed characters to appear in the wrong place.
- Scroll behavior in list views (Devices, Projects, Presets, Panels, Users) no longer produces erratic movement.
- Search fields in the path selector are now fully functional.
- PULSO page order now updates correctly as per client configuration.
- Panel objects with text now apply font size changes correctly when resizing with Shift.
- Fixed an issue where the minimum size of Panel objects was not updating correctly when modified via properties.
- Minor DSP and firmware stability improvements.


###########################################################################################################


EclerPLEX Release Notes, v1.02r24, 12 Jun 2026

Changes from last version, v1.02r20, 09 Jun 2026:

--------------------------------------------------------

Resolved software/firmware issues:

- Resolved an issue related to PEQ DSP blocks that could occasionally result in abnormal output levels.
- Fixed Reverse mode on Source selector control and Source selector volume events.
- Minor UI improvements to New event dialog.
- Corrected a bug that could cause presets not to load correctly or an unexpected reboot when loading a preset.
- Addressed inconsistencies when controlling Source selectors from a Panel dropdown.


###########################################################################################################


EclerPLEX Release Notes, v1.02r20, 09 Jun 2026

Changes from last version, v1.00r0, 31 Mar 2026:

Overview

This release brings significant improvements to event scheduling, panel controls, source selectors, clock synchronization, and overall system stability. Key highlights include enhanced daily event repetition handling, new DSP filter options, expanded panel object capabilities, and numerous bug fixes across firmware and web interface.


Device & System
- LCD health indicator - The front panel screen now displays a general health error indicator when system issues are detected. 
- Firmware update error handling - Unmanaged firmware update errors are now properly reported.

Network & Connectivity
- HTTPS display - The device host address now correctly shows HTTPS when applicable. 
- Network conflict detection - Added checking when NET1 and NET2 are configured on the same network range, with user notification. 
- PULSO connection fixes
        - Fixed PULSO not connecting to the correct IP when NET1 was disconnected. 
        - PULSO now correctly detects changes to the Workspace ID (e.g., after regeneration). 
        - Improved auto-login and pairing behavior for deleted guests. 
- Deep Dive stability - Resolved audio dropouts and high DSP usage that could occur when initiating Deep Dive remote access. 

Matrix & Source Selectors
- Ordered source selectors - Source selectors now support user-defined ordering, with a new reordering option in properties. 
- Source selectors - OutMix groups coexistence - Now you can combine them to replicate selector’s functionality across multiple outputs.
- Real-time updates - Fixed delayed updates in Groups and Source Selectors when changes were made from a second client.

DSP & Audio
- Noise gate on outputs - Noise Gate DSP filter is now also available on output strips.
- Digital input trim & polarity - Digital inputs now support trim adjustment; polarity handling has been improved. 
- Ducker hold time - Extended maximum ducker hold time to 60 seconds. 
- Clock synchronization - Reworked the clock sync algorithm for improved accuracy, especially when NTP is active. The system now adapts continuously to clock divergences. 
- CPU load threshold - Increased maximum allowed CPU load from 80% to 85%, reflecting performance improvements. 

Events
- Daily repetition fix - Resolved a bug preventing daily event repetitions from triggering correctly. The calendar monitor now advances properly after the current date. 
- Source selector support in events - Events can now trigger source selector actions using GPI/VGPI control. 
- Last action tracking - Refactored how events track and display the last executed action, ensuring accurate status across the interface. 
- GPI/VGPI improvements - Fixed polarity not being read correctly for VGPI triggers; properties canvas now displays accurate settings.

Panels
- Knob & Slider enhancements - Knobs and sliders can now control analog inputs gain and source selectors (selected element volume). 
- Button hold mode - Buttons now support a dedicated HOLD mode for momentary actions. 
- VU Meters - Added Pre and Post DSP options for VU meter signal monitoring. 
- Undo/Redo - Fixed some bugs related to undo and redo support. 
- Alignment & snapping - Improved alignment lines for rotated and multi-selected objects; optimized snap-to-object behavior. 
- Group handling - Fixed issues with group reordering, object duplication, pasting, and resizing. 
- Combo object - Added background color option to dropdown combo objects. 
- Text & font - Fixed attributes not updating in duplicated objects. 
- User menu - Corrected menu positioning, sizing, and presence for PULSO devices. 

Web Interface
- Project properties - Fixed issues where project properties did not display after deselecting a strip. 
- Dashboard updates - Dashboard cards now update reliably when changes occur on another client. 
- Log filtering - "Yesterday" is now the second date filter option for easier log review. 
- PEQ graph - X-axis now spans 10 Hz to 30 kHz; added Y-axis options. 
- List view - Fixed single-tap selection in list views. 
- Text controllers - Improved memory management and responsiveness for text input fields throughout the interface.

